Obstacle Avoiding



Car Design

2023

**Author : Sherif Ashraf Khadr**

Table of Contents

[Project Introduction 3](#_Toc135000892)

[Car Components 3](#_Toc135000893)

[Description 3](#_Toc135000894)

[Layered Architecture 5](#_Toc135000895)

[Mcal Layer 5](#_Toc135000896)

[Ecu Layer 6](#_Toc135000897)

[App Layer 6](#_Toc135000898)

[Common Layer 6](#_Toc135000899)

[Layered\_Architecture\_Figure 7](#_Toc135000900)

[High Level Design 8](#_Toc135000901)

[Drivers Documentation 8](#_Toc135000902)

[Mcal Layer 8](#_Toc135000903)

[1 - Dio Driver 8](#_Toc135000904)

[2 – External\_Interrupt 24](#_Toc135000905)

[3 – TIMERS 31](#_Toc135000906)

[Ecu Layer 45](#_Toc135000907)

[1 – Push Button 45](#_Toc135000908)

[2 – Dc Motor 50](#_Toc135000909)

[3 – Lcd 56](#_Toc135000910)

[4 – Keypad 68](#_Toc135000911)

# Project Introduction

## Car Components

1 - Atmega32 Microcontroller

2 - Four Motors (M1,M2,M3,M4)

3 - One Push Button To Change Direction Of Rotation

4 - Keypad Button 1 To Start

5 - Keypad Button 2 To Stop

6 - One Ultrasonic Sensor

7 - Lcd

## Description

1 - In First Start The Robot Will Wait For 2 Seconds To Choose The Default Direction Of Rotation Using The Push Button & Display On The Lcd User Can Choose Between Right & Left

2 - If No Obstacles Or Object Is Far Than 70 Centimetres Then The Robot Will Move Forward With 30% Speed For 5 Seconds & Then It Will Move With Speed Of 50% As Long As Was No Object Or Object Are Located At More Than 70 Centimetres distance

3 - If Object Located Between 30 & 70 Centimetres Then The Robot Will Decrease Its Speed To 30%

4 - If Object Located Between 20 & 30 Centimetres Then The Robot Will Stop & Rotates 90 Degrees To Right Or Left According To The Chosen Configuration

5 - If Object Located Less Than 20 Centimetres Then The Robot Will Stop Turn Direction To Backwards With Speed 30% Until The Distance Is Greater Than 20 And Less Than 30 Then Perform Point 4

6 - If Obstacles Surrounding The Robot In All Direction Without Finding Any Distance Greater Than 20 It Will Stop Robot Will Check Frequently Each 3 Seconds If Any Obstacles Was Removed Or Not And Move In The Furthest Object

# Layered Architecture

Layered architecture in embedded systems organizes software components into distinct layers, each with a specific responsibility and level of abstraction. The layers are arranged hierarchically, starting from the hardware layer, followed by MCAL, HAL and ending with the application layer. Layering provides benefits like modularity, scalability, and maintainability by separating software components into distinct layers with clear separation of concerns.

## Mcal Layer

Mcal is a layer in embedded systems that provides a standardized interface to the microcontroller hardware. It includes functions/drivers for controlling hardware peripherals and is critical for enabling higher-level software layers to be developed independently of the hardware platform.

## Ecu Layer

In a layered architecture for embedded systems, the ECU (Electronic Control Unit) layer sits above the MCAL layer and provides a higher-level, more application-specific interface for controlling the system's functions. It implements the system's primary functionality and interacts with the MCAL layer through well-defined APIs and interfaces. The ECU layer may also include functionality for managing system diagnostics, error handling, and communication with other ECUs or external systems.

## App Layer

In a layered architecture for embedded systems, the APP (Application) layer is responsible for providing the system's primary functionality and interacts with the lower layers through well-defined APIs and interfaces. It may include software components for implementing specific functions, managing system diagnostics, error handling, and communication with other systems.

## Common Layer

In a layered architecture for embedded systems, the common layers provide shared services and functionality used by multiple software components. They typically include components for managing system resources, configuration settings, and common functionality such as logging or debugging. Separating common functionality into distinct layers enables the system to function cohesively and be more modular and maintainable.

## Layered\_Architecture\_Figure

A picture containing text, screenshot, diagram, font

Description automatically generated

# High Level Design

# Drivers Documentation

## Mcal Layer

### 1 - Dio Driver

/\*

Enum : EN\_logic\_t

Description: Enumeration for the two possible logic states of a GPIO (General Purpose Input/Output)

pin on a micro-controller.

Members:

- GPIO\_LOGIC\_LOW : This member represents the logic level of a GPIO pin when it is set to low (0V).

- GPIO\_LOGIC\_HIGH : This member represents the logic level of a GPIO pin when it is set to high

(3.3V or 5V depending on the specific micro-controller).

Overall, the EN\_logic\_t enumeration provides a standardized way to represent and configure the logic

levels of GPIO pins on a micro-controller, making it easier to write and maintain software that interacts

with these pins.

\*/

typedef enum{

GPIO\_LOGIC\_LOW = 0,

GPIO\_LOGIC\_HIGH

}EN\_logic\_t;

/\*

Enum : EN\_direction\_t

Description: Enumeration for the two possible directions of a GPIO (General Purpose Input/Output)

pin on a micro-controller.

Members:

- GPIO\_DIRECTION\_INPUT : This member represents the direction of a GPIO pin when it is set to input mode, allowing it to receive and read external signals.

- GPIO\_DIRECTION\_OUTPUT : This member represents the direction of a GPIO pin when it is set to output mode, allowing it to send signals to external devices.

Overall, the EN\_direction\_t enumeration provides a standardized way to represent and configure the direction

of GPIO pins on a micro-controller, making it easier to write and maintain software that interacts

with these pins.

\*/

typedef enum

{

GPIO\_DIRECTION\_INPUT = 0,

GPIO\_DIRECTION\_OUTPUT

}EN\_direction\_t;

/\*

Enum : EN\_pin\_index\_t

Description : Enumeration for the index of each GPIO (General Purpose Input/Output) pin on a port.

Members:

- GPIO\_PIN0 : This member represents the index of the first GPIO pin on a port.

- GPIO\_PIN1 : This member represents the index of the second GPIO pin on a port.

- GPIO\_PIN2 : This member represents the index of the third GPIO pin on a port.

- GPIO\_PIN3 : This member represents the index of the fourth GPIO pin on a port.

- GPIO\_PIN4 : This member represents the index of the fifth GPIO pin on a port.

- GPIO\_PIN5 : This member represents the index of the sixth GPIO pin on a port.

- GPIO\_PIN6 : This member represents the index of the seventh GPIO pin on a port.

- GPIO\_PIN7 : This member represents the index of the eighth GPIO pin on a port.

Overall, the EN\_pin\_index\_t enumeration provides a standardized way to represent and identify each

GPIO pin on a port, making it easier to write and maintain software that interacts with these pins.

\*/

typedef enum

{

GPIO\_PIN0 = 0,

GPIO\_PIN1,

GPIO\_PIN2,

GPIO\_PIN3,

GPIO\_PIN4,

GPIO\_PIN5,

GPIO\_PIN6,

GPIO\_PIN7

}EN\_pin\_index\_t;

/\*

Enum : EN\_port\_index\_t

Description : Enumeration for the index of each GPIO (General Purpose Input/Output) port on a micro-controller.

Members :

- GPIO\_PORTA\_INDEX : This member represents the index of the first GPIO port on a micro-controller.

- GPIO\_PORTB\_INDEX : This member represents the index of the second GPIO port on a micro-controller.

- GPIO\_PORTC\_INDEX : This member represents the index of the third GPIO port on a micro-controller.

- GPIO\_PORTD\_INDEX : This member represents the index of the fourth GPIO port on a micro-controller.

Overall, the EN\_port\_index\_t enumeration provides a standardized way to represent and identify each

GPIO port on a micro-controller, making it easier to write and maintain software that interacts

with these ports and their associated pins.

\*/

typedef enum

{

GPIO\_PORTA\_INDEX = 0,

GPIO\_PORTB\_INDEX,

GPIO\_PORTC\_INDEX,

GPIO\_PORTD\_INDEX,

}EN\_port\_index\_t;

/\*

Struct : ST\_pin\_config\_t

Description : A structure that contains the configuration settings for a GPIO (General Purpose Input/Output)pin on a micro-controller.

Members:

- port : A 3-bit field that specifies the index of the GPIO port to which the pin belongs (0-3).

- pin : A 3-bit field that specifies the index of the GPIO pin on the port (0-7).

- direction : A 1-bit field that specifies the direction of the GPIO pin (input or output).

- logic : A 1-bit field that specifies the logic level of the GPIO pin (high or low).

Overall, the ST\_pin\_config\_t structure provides a standardized way to represent and configure the settings

for a single GPIO pin on a micro-controller, making it easier to write and maintain software that interacts

with these pins. The use of bit fields for the port, pin , direction , and logic members allows for

efficient use of memory and reduces the size of the structure. The Uchar8\_t type is likely a custom data

type defined in the software to represent an 8-bit unsigned character.

\*/

typedef struct

{

Uchar8\_t port : 3;

Uchar8\_t pin : 3;

Uchar8\_t direction : 1;

Uchar8\_t logic : 1;

}ST\_pin\_config\_t;

/\*

Function: GPIO\_pin\_direction\_intialize

Description: Initializes the direction of a GPIO pin on a micro-controller based on the pin configuration specified in the input parameter.

Parameters: \_pin\_config: A pointer to an instance of the ST\_pin\_config\_t struct that contains

the pin number, port number, pin logic on the pin and desired direction of the GPIO pin.

Return Type: Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

E\_OK : The function has completed successfully.

E\_NOT\_OK: The function has encountered an error and could not complete successfully.


Overall, the GPIO\_pin\_direction\_intialize function provides a way to initialize the direction of a GPIO pin

based on its configuration, allowing the software to set the direction of the pin

as needed for its specific functionality.

\*/

**Std\_ReturnType GPIO\_pin\_direction\_intialize(const ST\_pin\_config\_t \*\_pin\_config);**

****

/\*

Function: GPIO\_pin\_get\_direction\_status

Description: Gets the current direction status of a GPIO (General Purpose Input/Output) pin on a micro-controller based on the pin configuration specified in the input parameter.

Parameters:

- \_pin\_config : A pointer to an instance of the ST\_pin\_config\_t struct that contains the pin number,

port number,pin logic and desired direction of the GPIO pin.

- direction\_status : A pointer to a variable of type EN\_direction\_t where the current direction status of

the GPIO pin will be stored.

Return Type : Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:


- E\_OK : The function has completed successfully.

- E\_NOT\_OK : The function has encountered an error and could not complete successfully.

Overall, the GPIO\_pin\_get\_direction\_status function provides a way to retrieve the current direction status of a GPIO pin based on its configuration, allowing the software to check the pin's direction as needed.

\*/

**Std\_ReturnType GPIO\_pin\_get\_direction\_status(const ST\_pin\_config\_t \*\_pin\_config , EN\_direction\_t \*direction\_status);**



/\*

Function: GPIO\_pin\_write\_logic

Description : Writes the logic level of a GPIO (General Purpose Input/Output) pin on a micro-controller based on the pin configuration and desired logic level specified in the input parameters.

Parameters:

- \_pin\_config : A pointer to an instance of the ST\_pin\_config\_t struct that contains the pin number,

port number, pin logic and current direction of the GPIO pin.

- logic : The desired logic level to be written to the GPIO pin, either GPIO\_LOGIC\_LOW or GPIO\_LOGIC\_HIGH.

Return Type : Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

- E\_OK : The function has completed successfully.


- E\_NOT\_OK : The function has encountered an error and could not complete successfully.

Overall, the GPIO\_pin\_write\_logic function provides a way to write a logic level to a GPIO pin based on

its configuration, allowing the software to set the output of the pin as needed for its specific functionality.

\*/

**Std\_ReturnType GPIO\_pin\_write\_logic(const ST\_pin\_config\_t \*\_pin\_config , EN\_logic\_t logic);**



/\*

Function: GPIO\_pin\_read\_logic

Description: Reads the current logic level of a GPIO (General Purpose Input/Output) pin on a micro-controller based on the pin configuration specified in the input parameter.

Parameters:

- \_pin\_config : A pointer to an instance of the ST\_pin\_config\_t struct that contains the pin number,

port number, pin logic and current direction of the GPIO pin.

- logic\_status : A pointer to a variable of type EN\_logic\_t where the current logic level of the GPIO pin will be stored.

Return Type: Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:


- E\_OK : The function has completed successfully.

- E\_NOT\_OK : The function has encountered an error and could not complete successfully.

Overall, the GPIO\_pin\_read\_logic function provides a way to read the current logic level of a GPIO pin based on its configuration, allowing the software to check the input of the pin as needed for its specific functionality The current logic level is stored in the logic\_status parameter.

\*/

**Std\_ReturnType GPIO\_pin\_read\_logic(const ST\_pin\_config\_t \*\_pin\_config , EN\_logic\_t \*logic\_status);**



/\*

Function: GPIO\_pin\_toggle\_logic

Description: Toggles the logic level of a GPIO (General Purpose Input/Output) pin on a micro-controller based on the pin configuration specified in the input parameter.

Parameters:

- \_pin\_config : A pointer to an instance of the ST\_pin\_config\_t struct that contains the pin number,

port number, pin logic and current direction of the GPIO pin.

Return Type : Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

- E\_OK : The function has completed successfully.


- E\_NOT\_OK : The function has encountered an error and could not complete successfully.

Overall, the GPIO\_pin\_toggle\_logic function provides a way to toggle the logic level of a GPIO pin based on its configuration, allowing the software to change the output of the pin between high and low states as

needed for its specific functionality.

\*/

**Std\_ReturnType GPIO\_pin\_toggle\_logic(const ST\_pin\_config\_t \*\_pin\_config);**

/\*

Function: GPIO\_pin\_intialize

Description : Initializes a GPIO (General Purpose Input/Output) pin on a micro-controller based on the pin configuration specified in the input parameter.

Parameters:

- \_pin\_config : A pointer to an instance of the ST\_pin\_config\_t struct that contains the pin number,

port number, direction, and initial logic level of the GPIO pin.

Return Type : Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

- E\_OK : The function has completed successfully.

- E\_NOT\_OK : The function has encountered an error and could not complete successfully.


Overall, the GPIO\_pin\_intialize function provides a way to initialize a GPIO pin based

on its configuration, allowing the software to set the initial direction and logic level

of the pin as needed for its specific functionality.

\*/

**Std\_ReturnType GPIO\_pin\_intialize(const ST\_pin\_config\_t \*\_pin\_config);**

****

### 2 – External\_Interrupt

/\*

Enum: EN\_MCUCR\_REG\_BITS

Description: An enumeration that defines the bit fields for the `MCUCR` register on a micro-controller.

Members:

- MCUCR\_REG\_ISC00\_BITS : Represents the bit field for the `ISC00` bit of the `MCUCR` register.

- MCUCR\_REG\_ISC01\_BITS : Represents the bit field for the `ISC01` bit of the `MCUCR` register.

- MCUCR\_REG\_ISC10\_BITS : Represents the bit field for the `ISC10` bit of the `MCUCR` register.

- MCUCR\_REG\_ISC11\_BITS : Represents the bit field for the `ISC11` bit of the `MCUCR` register.

Overall, the EN\_MCUCR\_REG\_BITS enumeration provides a way to represent and manage the individual bit fields within the `MCUCR` register on a micro-controller in a standardized and easy-to-understand manner.By using this enumeration, the software can read and modify the individual bits within this register as needed for interrupt configuration and other purposes.

\*/

typedef enum

{

MCUCR\_REG\_ISC00\_BITS = 0,

MCUCR\_REG\_ISC01\_BITS,

MCUCR\_REG\_ISC10\_BITS,

MCUCR\_REG\_ISC11\_BITS

}EN\_MCUCR\_REG\_BITS;

/\*

Enum: EN\_MCUCSR\_REG\_BITS

Description: An enumeration that defines the bit fields for the `MCUCSR` register on a micro-controller.

Members:

- MCUCSR\_REG\_ISC2\_BITS : Represents the bit field for the `ISC2` bit of the `MCUCSR` register.

Overall, the EN\_MCUCSR\_REG\_BITS enumeration provides a way to represent and manage the individual bit fields within the `MCUCSR` register on a micro-controller in a standardized and easy-to-understand manner. By using this enumeration, the software can read and modify the individual bits within

this register as needed for interrupt configuration and other purposes.

\*/

typedef enum

{

MCUCSR\_REG\_ISC2\_BITS = 6,

}EN\_MCUCSR\_REG\_BITS;

/\*

Enum: EN\_GICR\_REG\_BITS

Description: An enumeration that defines the bit fields for the `GICR` register on a micro-controller.

Members:

- GICR\_REG\_INT2\_BITS : Represents the bit field for the `INT2` bit of the `GICR` register.

- GICR\_REG\_INT0\_BITS : Represents the bit field for the `INT0` bit of the `GICR` register.

- GICR\_REG\_INT1\_BITS : Represents the bit field for the `INT1` bit of the `GICR` register.

Overall, the EN\_GICR\_REG\_BITS enumeration provides a way to represent and manage the individual bit fields within the `GICR` register on a micro-controller in a standardized and easy-to-understand manner.

By using this enumeration, the software can read and modify the individual bits within this register as needed for interrupt configuration and other purposes.

\*/

typedef enum

{

GICR\_REG\_INT2\_BITS = 5,

GICR\_REG\_INT0\_BITS,

GICR\_REG\_INT1\_BITS

}EN\_GICR\_REG\_BITS;

/\*

Enum: EN\_GIFR\_REG\_BITS

Description: An enumeration that defines the bit fields for the `GIFR` register on a micro-controller.

Members:

- GIFR\_REG\_INTF2\_BITS : Represents the bit field for the `INTF2` bit of the `GIFR` register.

- GIFR\_REG\_INTF0\_BITS : Represents the bit field for the `INTF0` bit of the `GIFR` register.

- GIFR\_REG\_INTF1\_BITS : Represents the bit field for the `INTF1` bit of the `GIFR` register.

Overall, the EN\_GIFR\_REG\_BITS enumeration provides a way to represent and manage the individual bit fields within the `GIFR` register on a micro-controller in a standardized and easy-to-understand manner.

By using this enumeration, the software can read and modify the individual bits within this register as needed for interrupt handling and other purposes.

\*/

typedef enum

{

GIFR\_REG\_INTF2\_BITS = 5,

GIFR\_REG\_INTF0\_BITS,

GIFR\_REG\_INTF1\_BITS

}EN\_GIFR\_REG\_BITS;

/\*

Enum: EN\_EXT\_INTERRUPT\_Sense\_Control

Description: An enumeration that defines the possible sense control modes for external interrupts on a micro-controller.

Members:

- LOW\_LEVEL\_SENSE\_CONTROL : Represents the sense control mode where the interrupt is triggered when the input signal is at a low level.

- ANY\_LOGICAL\_SENSE\_CONTROL : Represents the sense control mode where the interrupt is triggered when there is any change in the logical state of the input signal.

- FALLING\_EDGE\_SENSE\_CONTROL : Represents the sense control mode where the interrupt is triggered when the input signal changes from a high level to a low level.

- RISING\_EDGE\_SENSE\_CONTROL : Represents the sense control mode where the interrupt is triggered when the input signal changes from a low level to a high level.

Overall, the EN\_EXT\_INTERRUPT\_Sense\_Control enumeration provides a way to represent and manage the different sense control modes for external interrupts on a micro-controller in a standardized and easy-to-understand manner. By using this enumeration, the software can configure and handle external interrupts based on the desired sense control mode for the specific input signal being used.

\*/

typedef enum

{

LOW\_LEVEL\_SENSE\_CONTROL = 0,

ANY\_LOGICAL\_SENSE\_CONTROL,

FALLING\_EDGE\_SENSE\_CONTROL,

RISING\_EDGE\_SENSE\_CONTROL

}EN\_EXT\_INTERRUPT\_Sense\_Control;

/\*

Enum: EN\_EXT\_INTERRUPTS

Description: An enumeration that defines the external interrupts available on a micro-controller.

Members:

- EXT0\_INTERRUPTS : Represents external interrupt 0.

- EXT1\_INTERRUPTS : Represents external interrupt 1.

- EXT2\_INTERRUPTS : Represents external interrupt 2.

Overall, the EN\_EXT\_INTERRUPTS enumeration provides a way to represent and manage the available external interrupts on a micro-controller in a standardized and easy-to-understand manner. By using this

enumeration, the software can configure and handle external interrupts based on the specific interrupt being used.

\*/

typedef enum

{

EXT0\_INTERRUPTS = 0,

EXT1\_INTERRUPTS,

EXT2\_INTERRUPTS

}EN\_EXT\_INTERRUPTS;

/\*

Struct: ST\_EXT\_INTERRUPTS\_CFG

Description: A structure that contains the configuration settings for an external interrupt on a micro-controller.

Members:

- INTERRUPT\_EXTERNAL\_HANDLER : A function pointer to the interrupt service routine (ISR) for the external interrupt(call-back function).

- EXTERNAL\_INTERRUPRT\_Number : An instance of the EN\_EXT\_INTERRUPTS enum that specifies the external interrupt number to be configured.

- EXTERNAL\_INTERRUPRT\_Sense\_Control : An instance of the EN\_EXT\_INTERRUPT\_Sense\_Control enum that specifies the sense control mode for the external interrupt.

Overall, the ST\_EXT\_INTERRUPTS\_CFG structure provides a way to represent and manage the configuration settings for an external interrupt on a micro-controller in a standardized and easy-to-understand manner. By using this structure, the software can configure and handle external interrupts based on the desired interrupt number and sense control mode, and execute the appropriate ISR when the interrupt is triggered.

\*/

typedef struct

{

void(\*INTERRUPT\_EXTERNAL\_HANDLER)(void);

EN\_EXT\_INTERRUPTS EXTERNAL\_INTERRUPRT\_Number;

EN\_EXT\_INTERRUPT\_Sense\_Control EXTERNAL\_INTERRUPRT\_Sense\_Control;

}ST\_EXT\_INTERRUPTS\_CFG;

/\*

Function: EXT\_vINTERRUPT\_Init

Description: Initializes an external interrupt on a micro-controller with the specified configuration settings.

Parameters:

- EXT\_INTx : A pointer to an ST\_EXT\_INTERRUPTS\_CFG struct that contains the configuration settings for the external interrupt.

Return Type: Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

- E\_OK : The function has completed successfully.

- E\_NOT\_OK : The function has encountered an error and could not complete successfully.

Overall, the EXT\_vINTERRUPT\_Init function provides a way to initialize an external interrupt on a


micro-controller with the desired configuration settings. By using this function, the software can set

up and handle external interrupts based on the specific interrupt number and sense control mode, and

execute the appropriate ISR when the interrupt is triggered.

\*/

**Std\_ReturnType EXT\_vINTERRUPT\_Init(const ST\_EXT\_INTERRUPTS\_CFG \*EXT\_INTx);**



/\*

Function: EXT\_vINTERRUPT\_Denit

Description: Deinitializes an external interrupt on a micro-controller with the specified configuration settings.

Parameters:

- EXT\_INTx : A pointer to an ST\_EXT\_INTERRUPTS\_CFG struct that contains the configuration settings for the external interrupt.

Return Type: Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

- E\_OK : The function has completed successfully.

- E\_NOT\_OK : The function has encountered an error and could not complete successfully.

Overall, the EXT\_vINTERRUPT\_Denit function provides a way to deinitialize an external


interrupt on a micro-controller with the desired configuration settings. By using this

function, the software can remove the interrupt and associated ISR, freeing up resources

and ensuring proper operation of the micro-controller.

\*/

**Std\_ReturnType EXT\_vINTERRUPT\_Denit(const ST\_EXT\_INTERRUPTS\_CFG \*EXT\_INTx);**

****

### 3 – TIMERS

#### **Timers With All Modes (Normal – Ctc – Pwm - Icu)**

/\*

Documentation for the Timer Channel Enum:

The enu\_TimerChannel typedef enum provides a list of options for different timer channels. The options are as follows:

TIMER0\_NORMAL: This option selects normal timer mode for Timer0.

TIMER0\_CTC: This option selects Clear Timer on Compare (CTC) mode for Timer0.

TIMER1\_NORMAL: This option selects normal timer mode for Timer1.

TIMER1\_CTC\_OCR: This option selects CTC mode for Timer1, using OCR1A as the comparison value.

TIMER1\_CTC\_ICR: This option selects CTC mode for Timer1, using ICR1 as the comparison value.

TIMER2\_NORMAL: This option selects normal timer mode for Timer2.

TIMER2\_CTC: This option selects CTC mode for Timer2.

\*/

**typedef enum{**

**TIMER0\_NORMAL,**

**TIMER0\_CTC,**

**TIMER1\_NORMAL,**

**TIMER1\_CTC\_OCR,**

**TIMER1\_CTC\_ICR,**

**TIMER2\_NORMAL,**

**TIMER2\_CTC**

**}enu\_TimerChannel;**

/\*

Documentation for the Prescale Modes Enum:

The enu\_prescale\_modes typedef enum provides a list of options for different prescale modes. The options are as follows:

TMR\_PRE\_NO\_CLK: This option selects no clock source for the timer, effectively stopping it.

TMR\_PRE\_0: This option selects the system clock with no prescaling.

TMR\_PRE\_8: This option selects the system clock divided by 8 as the clock source.

TMR\_PRE\_64: This option selects the system clock divided by 64 as the clock source.

TMR\_PRE\_256: This option selects the system clock divided by 256 as the clock source.

TMR\_PRE\_1024: This option selects the system clock divided by 1024 as the clock source.

TMR\_PRE\_EXT\_FALLING: This option selects an external clock source with falling edge triggering as the clock source.

TMR\_PRE\_EXT\_RISING: This option selects an external clock source with rising edge triggering as the clock source.

TMR\_PRE\_32: This option selects the system clock divided by 32 as the clock source.

TMR\_PRE\_128: This option selects the system clock divided by 128 as the clock source.

\*/

**typedef enum{**

**TMR\_PRE\_NO\_CLK,**

**TMR\_PRE\_0,**

**TMR\_PRE\_8,**

**TMR\_PRE\_64,**

**TMR\_PRE\_256,**

**TMR\_PRE\_1024,**

**TMR\_PRE\_EXT\_FALLING,**

**TMR\_PRE\_EXT\_RISING,**

**TMR\_PRE\_32,**

**TMR\_PRE\_128**

**}enu\_prescale\_modes;**

/\*

Documentation for the Timer Toggle Mode Enum:

The enu\_TimerToggleMode typedef enum provides a list of options for different timer toggle modes. The options are as follows:

TMR\_OCMode: This option selects Output Compare (OC) mode for the timer.

TMR\_InterruptMode: This option selects Interrupt mode for the timer.

\*/

**typedef enum{**

**TMR\_OCMode,**

**TMR\_InterruptMode**

**}enu\_TimerToggleMode;**

/\*

Documentation for the Timer Output Compare Mode Enum:

The enu\_TimerOCMode typedef enum provides a list of options for different timer output compare modes. The options are as follows:

OC\_Disconnected: This option disconnects the output compare pin from the timer.

OC\_Toggle: This option toggles the output compare pin on a compare match.

OC\_Clear: This option clears the output compare pin on a compare match.

OC\_Set: This option sets the output compare pin on a compare match.

\*/

**typedef enum{**

**OC\_Disconnected,**

**OC\_Toggle,**

**OC\_Clear,**

**OC\_Set**

**}enu\_TimerOCMode;**

/\*

Function Description: The TMR\_vInit function initializes and sets up a timer with the settings specified in the input TMR\_cfg\_t configuration structure. Once the timer is initialized and set up, it can be used for various timing applications such as measuring elapsed time, generating interrupts at specified intervals, or controlling the timing of other operations in a system.


Function Parameters:

- TMR: a pointer to a TMR\_cfg\_t structure containing the desired timer channel, prescale mode, toggle mode, and output compare mode settings.

Function Return Type: void

\*/

**void TMR\_vInit(const TMR\_cfg\_t \*TMR);**



/\*

Function Name: TMR\_vStop

Function Description: The TMR\_vStop function is used to stop a timer that is configured with the settings specified in the input TMR\_cfg\_t configuration structure.


Function Parameters:

- TMR: a pointer to a TMR\_cfg\_t structure containing the settings for the timer to be stopped.

Function Return Type: void

\*/

**void TMR\_vStop(const TMR\_cfg\_t \*TMR);**

****

/\*

Function Name: TMR\_vSetICRValue

Function Description: The TMR\_vSetICRValue function sets the Input Capture Register (ICR) value for the timer that is configured with the settings specified in the input TMR\_cfg\_t configuration structure.

Function Parameters:

TMR: a pointer to a TMR\_cfg\_t structure containing the settings for the timer to be configured.

Copy\_u16ICRValue: a 16-bit unsigned integer value that specifies the value to which the ICR register will be set.

Function Return Type: void

\*/

**void TMR\_vSetICRValue(const TMR\_cfg\_t \*TMR, u16 Copy\_u16ICRValue);**

****

/\*

Function Name: TMR\_vSetOCRValue

Function Description: The TMR\_vSetOCRValue function sets the Output Compare Register (OCR) value for the timer that is configured with the settings specified in the input TMR\_cfg\_t configuration structure.

Function Parameters:


TMR: a pointer to a TMR\_cfg\_t structure containing the settings for the timer to be configured.

Copy\_u16OCRValue: a 16-bit unsigned integer value that specifies the value to which the OCR register will be set.

Function Return Type: void

\*/

**void TMR\_vSetOCRValue(const TMR\_cfg\_t \*TMR, u16 Copy\_u16OCRValue);**



/\*

Function Name: TMR\_vSetTCNTValue

Function Description: The TMR\_vSetTCNTValue function sets the Timer/Counter Register (TCNT) value for the timer that is configured with the settings specified in the input TMR\_cfg\_t configuration structure.

Function Parameters:


TMR: a pointer to a TMR\_cfg\_t structure containing the settings for the timer to be configured.

Copy\_u16TCNTValue: a 16-bit unsigned integer value that specifies the value to which the TCNT register will be set.

Function Return Type: void

\*/

**void TMR\_vSetTCNTValue(const TMR\_cfg\_t \*TMR, u16 Copy\_u16TCNTValue);**

****

/\*

Function Name: TMR\_vStartTimer

Function Description: The TMR\_vStartTimer function starts the timer that is configured with the settings specified in the input TMR\_cfg\_t configuration structure.


Function Parameters:

TMR: a pointer to a TMR\_cfg\_t structure containing the settings for the timer to be started.

Function Return Type: void

\*/

**void TMR\_vStartTimer(const TMR\_cfg\_t \*TMR);**



## Ecu Layer

### 1 – Push Button

/\*

Enum: EN\_PUSH\_BTN\_state\_t

Description : An enumeration that defines two possible states for a push button: pressed or released.

Members:

- PUSH\_BTN\_STATE\_PRESSED : Represents the state of a push button when it is pressed down or activated.

- PUSH\_BTN\_STATE\_RELEASED : Represents the state of a push button when it is not pressed or deactivated.

Overall, the EN\_PUSH\_BTN\_state\_t enumeration provides a way to represent the two possible states of a push button in a standardized and easy-to-understand manner. By using this enumeration, the software can check the state of a push button and take appropriate action based on whether it is pressed or released.

\*/

**typedef enum**

**{**

**PUSH\_BTN\_STATE\_PRESSED = 0,**

**PUSH\_BTN\_STATE\_RELEASED**

**}EN\_PUSH\_BTN\_state\_t;**

/\*

Enum: EN\_PUSH\_BTN\_active\_t

Description: An enumeration that defines two possible active states for a push button: pull-up or pull-down.

Members:

- PUSH\_BTN\_PULL\_UP : Represents the active state of a push button when it is connected to a pull-up resistor. In this state, the button is normally open and the pull-up resistor pulls the voltage of the pin to a high state.

- PUSH\_BTN\_PULL\_DOWN : Represents the active state of a push button when it is connected to a pull-down resistor. In this state, the button is normally closed and the pull-down resistor pulls the voltage of the pin to a low state.

Overall, the EN\_PUSH\_BTN\_active\_t enumeration provides a way to represent the two possible active states of a push button in a standardized and easy-to-understand manner. By using this enumeration, the software can determine the active state of a push button and configure the pin accordingly.

\*/

**typedef enum**

**{**

**PUSH\_BTN\_PULL\_UP = 0,**

**PUSH\_BTN\_PULL\_DOWN**

**}EN\_PUSH\_BTN\_active\_t;**

/\*

Struct : ST\_PUSH\_BTN\_t

Description : A structure that contains the configuration and current state information for a push button.

Members:

- PUSH\_BTN\_pin : An instance of the ST\_pin\_config\_t struct that contains the configuration settings

for the pin used by the push button.

- PUSH\_BTN\_state : An instance of the EN\_PUSH\_BTN\_state\_t enum that represents the current state of

the push button (pressed or released).

- PUSH\_BTN\_connection : An instance of the EN\_PUSH\_BTN\_active\_t enum that represents the active state of the push button (pull-up or pull-down).

Overall, the ST\_PUSH\_BTN\_t structure provides a standardized way to represent and manage the configuration and state information for a push button on a micro-controller. By using this structure, the software can easily read the current state of the push button and take appropriate action based on its configuration and connection type. The use of enums for the state and connection fields allows for consistent and easy-to-understand representation of these values.

\*/

**typedef struct**

**{**

**ST\_pin\_config\_t PUSH\_BTN\_pin;**

**EN\_PUSH\_BTN\_state\_t PUSH\_BTN\_state;**

**EN\_PUSH\_BTN\_active\_t PUSH\_BTN\_connection;**

**}ST\_PUSH\_BTN\_t;**

/\*

Function: PUSH\_BTN\_intialize

Description: Initializes a push button based on the configuration settings specified in the input parameter.

Parameters:

- btn : A pointer to an ST\_PUSH\_BTN\_t struct that contains the configuration settings for the push button.

Return Type: Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

- E\_OK : The function has completed successfully.

- E\_NOT\_OK : The function has encountered an error and could not complete successfully.


Overall, the PUSH\_BTN\_intialize function provides a way to initialize a push button based on the specified

configuration settings. By using this function, the software can ensure that the pin used by the push button

is configured correctly and the push button is ready for use.

\*/

**Std\_ReturnType PUSH\_BTN\_intialize(const ST\_PUSH\_BTN\_t \*btn);**



/\*

Function : PUSH\_BTN\_read\_state

Description : Reads the current state of a push button and returns its value.

Parameters:

- btn : A pointer to an ST\_PUSH\_BTN\_t struct that contains the configuration settings and current state

information for the push button.

- btn\_state : A pointer to an EN\_PUSH\_BTN\_state\_t enum where the current state of the push button will be stored.

Return Type : Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

- E\_OK : The function has completed successfully.

- E\_NOT\_OK : The function has encountered an error and could not complete successfully.


Overall, the PUSH\_BTN\_read\_state function provides a way to read the current state of a push button and return

its value. By using this function, the software can determine whether the push button is currently pressed or

released and take appropriate action based on its state.

\*/

**Std\_ReturnType PUSH\_BTN\_read\_state(const ST\_PUSH\_BTN\_t \*btn , EN\_PUSH\_BTN\_state\_t \*btn\_state);**

****

### 2 – Dc Motor

/\*

The `dc\_motor\_t` structure is used to specify the pin assignments for a DC motor in a microcontroller-based system. Its members are defined as follows:

- `motor\_port`: a 2-bit bit-field that specifies the port to which the DC motor is connected.

- `motor\_pin1`: a 3-bit bit-field that specifies the first pin of the DC motor.

- `motor\_pin2`: a 3-bit bit-field that specifies the second pin of the DC motor.

This configuration structure allows for easy and efficient assignment of pin assignments for a DC motor in embedded systems, using the specified port and pin numbers.

\*/

**typedef struct{**

**u8 motor\_port :2;**

**u8 motor\_pin1 :3;**

**u8 motor\_pin2 :3;**

**}dc\_motor\_t;**

/\*

Function Name: DC\_MOTOR\_vInit

Function Description: The DC\_MOTOR\_vInit function is used to initialize the pins and settings for a DC motor connected to a microcontroller-based system.


Function Parameters:

\_MOTOR: a pointer to a dc\_motor\_t structure containing the pin assignments and configuration settings for the DC motor.

Function Return Type: void

\*/

**void DC\_MOTOR\_vInit(const dc\_motor\_t \*\_MOTOR);**

****

/\*

Function Name: DC\_MOTOR\_Turn\_Off

Function Description: The DC\_MOTOR\_Turn\_Off function is used to turn off a DC motor that is connected to a microcontroller-based system.


Function Parameters:

\_MOTOR: a pointer to a dc\_motor\_t structure containing the pin assignments and configuration settings for the DC motor.

Function Return Type: void

\*/

**void DC\_MOTOR\_Turn\_Off(const dc\_motor\_t \*\_MOTOR);**

****

/\*

Function Name: DC\_MOTOR\_Turn\_On

Function Description: The DC\_MOTOR\_Turn\_On function is used to turn on a DC motor that is connected to a microcontroller-based system.


Function Parameters:

\_MOTOR: a pointer to a dc\_motor\_t structure containing the pin assignments and configuration settings for the DC motor.

Function Return Type: void

\*/

**void DC\_MOTOR\_Turn\_On(const dc\_motor\_t \*\_MOTOR);**

****

### 3 – Lcd

/\*

The LCD\_4bit\_cfg structure is a configuration structure used to specify the pin assignments for a 4-bit mode LCD in a microcontroller-based system. Its members are defined as follows:

LCD\_PORT: an unsigned 8-bit integer that specifies the port to which the LCD is connected. This member is a bit-field that is 2 bits wide.

LCD\_RS\_PIN: an unsigned 8-bit integer that specifies the register select (RS) pin of the LCD. This member is a bit-field that is 3 bits wide.

LCD\_RW\_PIN: an unsigned 8-bit integer that specifies the read/write (RW) pin of the LCD. This member is a bit-field that is 3 bits wide.

LCD\_EN\_PIN: an unsigned 8-bit integer that specifies the enable (EN) pin of the LCD. This member is a bit-field that is 3 bits wide.

LCD\_D4\_PIN: an unsigned 8-bit integer that specifies the data 4 (D4) pin of the LCD. This member is a bit-field that is 3 bits wide.

LCD\_D5\_PIN: an unsigned 8-bit integer that specifies the data 5 (D5) pin of the LCD. This member is a bit-field that is 3 bits wide.

LCD\_D6\_PIN: an unsigned 8-bit integer that specifies the data 6 (D6) pin of the LCD. This member is a bit-field that is 3 bits wide.

LCD\_D7\_PIN: an unsigned 8-bit integer that specifies the data 7 (D7) pin of the LCD. This member is a bit-field that is 3 bits wide.

By using this configuration structure, you can easily specify the pin assignments for a 4-bit mode LCD in your system. The exact implementation of the LCD\_4bit\_cfg structure will depend on the specific hardware and software platform being used, as well as the requirements of the application.

\*/

**typedef struct{**

**u8 LCD\_PORT :2;**

**u8 LCD\_RS\_PIN :3;**

**u8 LCD\_RW\_PIN :3;**

**u8 LCD\_EN\_PIN :3;**

**u8 LCD\_D4\_PIN :3;**

**u8 LCD\_D5\_PIN :3;**

**u8 LCD\_D6\_PIN :3;**

**u8 LCD\_D7\_PIN :3;**

**}LCD\_4bit\_cfg;**

/\*

Function Name: LCD\_4bit\_vInit

Function Description: The LCD\_4bit\_vInit function is used to initialize the pins and settings for a 4-bit mode LCD connected to a microcontroller-based system.


Function Parameters:

PTR\_LCD: a pointer to an LCD\_4bit\_cfg structure containing the pin assignments and configuration settings for the 4-bit mode LCD.

Function Return Type: void

\*/

**void LCD\_4bit\_vInit(const LCD\_4bit\_cfg \*PTR\_LCD);**

****

/\*

Function Name: LCD\_4bit\_vSendCmd

Function Description: The LCD\_4bit\_vSendCmd function is used to send a command to an LCD in 4-bit mode.

Function Parameters:


PTR\_LCD: a pointer to an LCD\_4bit\_cfg structure containing the pin assignments and configuration settings for the 4-bit mode LCD.

Copy\_u8Cmd: an 8-bit unsigned integer that specifies the command to be sent to the LCD.

Function Return Type: void

\*/

**void LCD\_4bit\_vSendCmd(const LCD\_4bit\_cfg \*PTR\_LCD, u8 Copy\_u8Cmd);**

****

/\*

Function Name: LCD\_4bit\_vSendChar

Function Description: The LCD\_4bit\_vSendChar function is used to send a character to an LCD in 4-bit mode.

Function Parameters:


PTR\_LCD: a pointer to an LCD\_4bit\_cfg structure containing the pin assignments and configuration settings for the 4-bit mode LCD.

Copy\_u8Char: an 8-bit unsigned integer that specifies the character to be sent to the LCD.

Function Return Type: void

\*/

**void LCD\_4bit\_vSendChar(const LCD\_4bit\_cfg \*PTR\_LCD, u8 Copy\_u8Char);**

****

/\*

Function Name: LCD\_4bit\_vSendChar\_pos

Function Description: The LCD\_4bit\_vSendChar\_pos function is used to send a character to a specific position on an LCD in 4-bit mode.

Function Parameters:

PTR\_LCD: a pointer to an LCD\_4bit\_cfg structure containing the pin assignments and configuration settings for the 4-bit mode LCD.

Copy\_u8Char: an 8-bit unsigned integer that specifies the character to be sent to the LCD.


row: an 8-bit unsigned integer that specifies the row (0 or 1) of the LCD where the character should be displayed.

column: an 8-bit unsigned integer that specifies the column (0 to 15) of the LCD where the character should be displayed.

Function Return Type: void

\*/

**void LCD\_4bit\_vSendChar\_pos(const LCD\_4bit\_cfg \*PTR\_LCD, u8 Copy\_u8Char, u8 row, u8 column);**

****

/\*

Function Name: LCD\_4bit\_vSendString

Function Description: The LCD\_4bit\_vSendString function is used to send a string of characters to an LCD in 4-bit mode.

Function Parameters:


PTR\_LCD: a pointer to an LCD\_4bit\_cfg structure containing the pin assignments and configuration settings for the 4-bit mode LCD.

Copy\_u8String: a pointer to an array of 8-bit unsigned integers that contains the string to be sent to the LCD.

Function Return Type: void

\*/

**void LCD\_4bit\_vSendString(const LCD\_4bit\_cfg \*PTR\_LCD, u8 \*Copy\_u8String);**

****

/\*

Function Name: LCD\_4bit\_vSendString\_pos

Function Description: The LCD\_4bit\_vSendString\_pos function is used to send a string of characters to a specific position on an LCD in 4-bit mode.

Function Parameters:

PTR\_LCD: a pointer to an LCD\_4bit\_cfg structure containing the pin assignments and configuration settings for the 4-bit mode LCD.

Copy\_u8String: a pointer to an array of 8-bit unsigned integers that contains the string to be sent to the LCD.


row: an 8-bit unsigned integer that specifies the row (0 or 1) of the LCD where the string should be displayed.

column: an 8-bit unsigned integer that specifies the column (0 to 15) of the LCD where the string should start.

Function Return Type: void

\*/

**void LCD\_4bit\_vSendString\_pos(const LCD\_4bit\_cfg \*PTR\_LCD, u8 \*Copy\_u8String, u8 row, u8 column);**

****

/\*

Function Name: LCD\_4bit\_vSendNumber

Function Description: The LCD\_4bit\_vSendNumber function is used to send a 16-bit unsigned integer as a decimal number to an LCD in 4-bit mode.

Function Parameters:


PTR\_LCD: a pointer to an LCD\_4bit\_cfg structure containing the pin assignments and configuration settings for the 4-bit mode LCD.

Copy\_u16Number: a 16-bit unsigned integer that contains the decimal number to be sent to the LCD.

Function Return Type: void

\*/

**void LCD\_4bit\_vSendNumber(const LCD\_4bit\_cfg \*PTR\_LCD, u16 Copy\_u16Number);**

****

/\*

Function Name: LCD\_4bit\_SetCursorPosition

Function Description: The LCD\_4bit\_SetCursorPosition function is used to set the cursor position of an LCD in 4-bit mode.

Function Parameters:

PTR\_LCD: a pointer to an LCD\_4bit\_cfg structure containing the pin assignments and configuration settings for the 4-bit mode LCD.


column: an 8-bit unsigned integer that specifies the column (0 to 15) of the LCD where the cursor should be moved.

row: an 8-bit unsigned integer that specifies the row (0 or 1) of the LCD where the cursor should be moved.

Function Return Type: void

\*/

**void LCD\_4bit\_SetCursorPosition(const LCD\_4bit\_cfg \*PTR\_LCD, u8 column, u8 row);**

****

### 4 – Keypad

/\*

Struct: ST\_KEYPAD\_cfg\_t

Description: A structure that contains the configuration settings for a keypad or matrix keyboard with a

specific number of rows and columns.

Members:

- KEYPAD\_arrRow[KEYPAD\_ROWS\_SIZE] : An array of ST\_pin\_config\_t structs that contains the configuration settings for the pins used as the rows of the keypad. The size of the array is specified by the KEYPAD\_ROWS\_SIZE macro.

- KEYPAD\_arrColumns[KEYPAD\_COLUMNS\_SIZE]: An array of ST\_pin\_config\_t structs that contains the configuration settings for the pins used as the columns of the keypad. The size of the array is specified by the KEYPAD\_COLUMNS\_SIZE macro.

Overall, the ST\_KEYPAD\_cfg\_t structure provides a structured and organized way to configure the pins used by a keypad or matrix keyboard. By using this structure, the software can ensure that the pins are configured correctly for their intended use, which can help to simplify the code and make it easier to understand. The use of arrays of ST\_pin\_config\_t structs allows for the configuration of multiple pins in a single structure, reducing the amount of code needed to configure the keypad or matrix keyboard.

\*/

**typedef struct**

**{**

**ST\_pin\_config\_t KEYPAD\_arrRow[KEYPAD\_ROWS\_SIZE];**

**ST\_pin\_config\_t KEYPAD\_arrColumns[KEYPAD\_COLUMNS\_SIZE];**

**}ST\_KEYPAD\_cfg\_t;**

/\*

Function : KEYPAD\_init

Description : Initializes a keypad or matrix keyboard based on the configuration settings specified in the input parameter.

Parameters :

- \_keypad : A pointer to an ST\_KEYPAD\_cfg\_t struct that contains the configuration pin settings for the keypad or matrix keyboard.

Return Type: Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

- E\_OK : The function has completed successfully.

- E\_NOT\_OK : The function has encountered an error and could not complete successfully.


Overall, the KEYPAD\_init function provides a way to initialize a keypad or matrix keyboard based on the

specified configuration settings. By using this function, the software can ensure that the pins are configured

correctly and the keypad or matrix keyboard is ready for use.

\*/

**Std\_ReturnType KEYPAD\_init(ST\_KEYPAD\_cfg\_t \*\_keypad);**



/\*

Function : KEYPAD\_scaningPressedBtn

Description : Scans the keypad or matrix keyboard for any pressed buttons and returns the value of the pressed button.

Parameters :

- \_keypad : A pointer to an ST\_KEYPAD\_cfg\_t struct that contains the configuration pin settings for the keypad or matrix keyboard.

- pressedBtnVal : A pointer to an 8-bit unsigned character where the value of the pressed button will be stored.

Return Type : Std\_ReturnType. This is a standard type used in AUTOSAR (Automotive Open System Architecture) software development to indicate the success or failure of a function call.

The possible return values for this function are:

- E\_OK : The function has completed successfully.

- E\_NOT\_OK : The function has encountered an error and could not complete successfully.

Overall, the KEYPAD\_scaningPressedBtn function provides a way to scan the keypad or matrix keyboard for any pressed buttons and retrieve the value of the pressed button. By using this function, the software can detect which button has been pressed and take appropriate action based on the button value.

\*/

**Std\_ReturnType KEYPAD\_scaningPressedBtn(ST\_KEYPAD\_cfg\_t \*\_keypad , Uchar8\_t \*pressedBtnVal);**

